CALA | Call to subroutine addressed by ACCL
CALAD | Delayed call to subroutine addressed by ACCL
CALL | Call to subroutine unconditionally
CALLD | Delayed call to subroutine unconditionally
CC | Call to subroutine conditionally
CCD | Delayed call to subroutine conditionally
CLRC | Clear overflow mode (OVM) bit Clear sign extension mode (SXM) bit Clear hold mode (HM) bit Clear test/control (TC) bit Clear carry (C) bit Clear configuration control (CNF) bit Clear interrupt mode (INTM) bit Clear external flag (XF) pin
CMPL | 1s complement ACC
CMPR | Compare AR with ARCR as specified by CM bits
CPL | Compare data memory value with DBMR
CRGT | Store ACC in ACCB if ACC > ACCB
CRLT | Store ACC in ACCB if ACC < ACCB