LACB | Load ACC to ACCB
LACC | Load data memory value, with left shift, to ACC Load long immediate, with left shift, to ACC Load data memory value, with left shift of 16, to ACC
LACL | Load data memory value to ACCL; zero ACCH Load short immediate to ACCL; zero ACCH
LACT | Load data memory value, with left shift specified by TREG1, to ACC
LAMM | Load contents of memory mapped register to ACCL; zero ACCH
LAR | Load data memory value to Arx Load short immediate to Arx Load long immediate to Arx
LDP | Load data memory value to DP bits Load short immediate to DP bits
LMMR | Load data memory value to memory-mapped register
LPH | Load data memory value to PREG high byte
LST | Load data memory value to ST0 Load data memory value to ST1
LT | Load data memory value to TREG0
LTA | Load data memory value to TREG0; add PREG, with shift specified by PM bits, to ACC
LTD | Load data memory value to TREG0; add PREG, with shift specified by PM bits, to ACC; and move data
LTP | Load data memory value to TREG0; store PREG, with shift specified by PM bits, in ACC
LTS | Load data memory value to TREG0; subtract PREG, with shift specified by PM bits, from ACC