B | Branch unconditionally to program memory location
BACC | Branch to program memory location specified by ACCL
BACCD | Delayed branch to program memory location specified by ACCL
BANZ | Branch to program memory location if AR not zero
BANZD | Delayed branch to program memory location if AR not zero
BCND | Branch conditionally to program memory location
BCNDD | Delayed branch conditionally to program memory location
BD | Delayed branch conditionally to program memory location
BIT | Test bit
BITT | Test bit specified by TREG2
BLDD | Block move from data to data memory Block move from data to data memory with destination address long immediate Block move from data to data memory with source address in BMAR Block move from data to data memory with destination address in BMAR
BLDP | Block move from data to program memory with destination address in BMAR
BLPD | Block move from program to data memory with source address in BMAR Block move from program to data memory with source address long immediate
BSAR | Barrel-shift ACC right