ABS | Absolute value of ACC; zero carry bit
ADCB | Add ACCB and carry bit to ACC
ADD | Add data memory value, with left shift, to ACC Add data memory value, with left shift of 16, to ACC Add short immediate to ACC Add long immediate, with left shift, to ACC
ADDB | Add ACCB to ACC
ADDC | Add data memory value and carry bit to ACC with sign extension suppressed
ADDS | Add data memory value to ACC with sign extension suppressed
ADDT | Add data memory value, with left shift specified by TREG1, to ACC
ADRK | Add short immediate to AR
AND | AND data memory value with ACCL; zero ACCH AND long immediate, with left shift, with ACC AND long immediate, with left shift of 16, with ACC
ANDB | AND ACCB with ACC Barrel-shift ACC right
APL | AND data memory value with DBMR, and store result in data memory location AND data memory value with long immediate and store result in data memory location
APAC |