XC | Execute next instruction(s) conditionally
XOR | Exclusive-OR data memory value with ACCL Exclusive-OR long immediate, with left shift of 16, with ACC Exclusive-OR long immediate, with left shift, with ACC
XORB | Exclusive-OR ACCB with ACC
XPL | Exclusive-OR data memory value with DBMR and store result in data memory location Exclusive-OR data memory value with long immediate and store result in data memory location