Conditional Call

    The CC (conditional call) is a 2-word instruction. The CC instruction operates

    like the BCND except that the PC pointing to the instruction following the CC

    is pushed onto the stack. Thus, the return (RET) operation can pop the stack

    to return to the calling sequence. A subroutine or function can have multiple

    return paths depending on the data being processed.